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1. Power the machine down.
2. Locate the particulate filters in the photos.  They are downward facing silver cylindrical tubes. One is attached to the AC vessel, and the other is located near the floor of the unit after the CO2 compressor.  
3. Depressurize the AC vessel using one of the ball valves on the vessel.
4. Unscrew the cylindrical stainless bottom piece.  It will be secured strongly.
5. You will see a small white filter resting on a spool.  Carefully remove the filter.
6. Remove this filter and inspect it for damage. If it is falling apart or pieces break off, please notify Earthly to send you replacement filters.
7. Gently rinse your filter under cool water and put it on a paper towel to dry.  
8. Once it is dry, replace the filter on the spool, and screw the cylindrical housing back on.
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