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O2 GOOD INLET VALVE OPEN
SYSTEM ON
CHILLER SYSTEM ON
3
2
113.5 psi
15/22/30/60


200.0lbs
0.0-0.9%
140.5 F
450.0 F
-35.1 F
145 – 150 psi
150 – 155 psi
155 – 160 psi

0.5 – 3.5 psi
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PRESSURES TEMPERATURES SENSORS ALARMS AND WARNINGS
INLET P COMP OUT T INLET 02 Unit Shut Down: Check Data Tab
12.34 PST 123.4 F 12.34 %

COMP OUT P HEATER OUT T| | DEWAR LEVEL
123.45 PST 123.4 F 123.4 %

fictivated Carbon Change Required

CHILLER IN P| [cHILLER ouT T| | coMP SPEED
123.45 PSI| || -1284.5 F 2t Compressor Maintenance Required

DEWER P AIR GO P | lieater Shut Down: Check Data Tab
123.45 PSI 123.45 PSI
10 to 20 Liquid CO2 Teft in Dewa

TOTAL C02 CAPTURED

PROCESS STATUS NOTIFICATION 1234567890 Tbs
HMI Version
4.01
RUNTIME HOURS PLC Version
12345 Hr 12.3
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