No Shutdown alert

Call Support

Unplug unit and reset breakers

No. Breakers aren’t tripped

Yes, breakers are tripped

Check breakers in front panel

Press ‘Reset’ on HMI

Yes, Shutdown alert.

Check For Shutdown on HMI

No

YesY

Compressor Running?

Wait for Inlet Pressure > 0.5 PSI

No

YesY

Inlet Pressure Above 0.5 PSI

Wait for O2% to drop below 0.09%

No

YesY

O2% Below 0.09%

Open Dewar Valves

No

YesY

Dewar Valves Open

CiCi Hooked Up To Fermentation

Call Support

Shutdown the unit and unplug from wall; Wait 30 seconds and plug back in

NoY

YesY

YesY

Is the chiller running?

NoY

YesY

Is ‘Heater’ Digital Display showing numbers?

NoY

YesY

Is Chiller Temp. Dropping?

NoY

YesY

Chiller On?

NoY

YesY

Wait for pressures to build

Compressor and Chiller Pressure above 145 psi?